<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
</package>
<package name="POWER_JACK_SLOT">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="TO-252">
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4001-KIT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="5V_EXT" library="SparkFun-Connectors" package="1X06_LONGPADS" value=""/>
<element name="GND_EXT" library="SparkFun-Connectors" package="1X06_LONGPADS" value=""/>
<element name="3V3" library="SparkFun-Connectors" package="1X06_LONGPADS" value=""/>
<element name="U$1" library="SparkFun-PowerIC" package="SOT223" value="LD111733"/>
<element name="C3O" library="fab" package="C1206FAB" value="10 uF"/>
<element name="C3I" library="fab" package="C1206FAB" value="100 nF"/>
<element name="J2" library="SparkFun-Connectors" package="POWER_JACK_SLOT" value="POWER_JACKSLT">
<attribute name="PROD_ID" value="PRT-00119"/>
</element>
<element name="78M05" library="SparkFun-PowerIC" package="TO-252" value="+12v">
<attribute name="PROD_ID" value="VREG-12370"/>
</element>
<element name="C5O" library="fab" package="C1206FAB" value="0.1 uF"/>
<element name="C50" library="fab" package="C1206FAB" value=""/>
<element name="C51" library="fab" package="C1206FAB" value=""/>
<element name="C52" library="fab" package="C1206FAB" value="0.1 uF"/>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4001-KIT" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="GND_EXT" pad="6"/>
<contactref element="GND_EXT" pad="5"/>
<contactref element="GND_EXT" pad="4"/>
<contactref element="GND_EXT" pad="3"/>
<contactref element="GND_EXT" pad="2"/>
<contactref element="GND_EXT" pad="1"/>
<contactref element="J2" pad="GND@1"/>
<contactref element="J2" pad="GND@2"/>
<contactref element="78M05" pad="3"/>
<contactref element="C5O" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="C52" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="C3I" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="3V">
<contactref element="3V3" pad="6"/>
<contactref element="3V3" pad="5"/>
<contactref element="3V3" pad="4"/>
<contactref element="3V3" pad="3"/>
<contactref element="3V3" pad="2"/>
<contactref element="3V3" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="C3I" pad="1"/>
<contactref element="C3O" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="78M05" pad="1"/>
<contactref element="C51" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="C52" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="U$1" pad="3"/>
<contactref element="C3O" pad="2"/>
</signal>
<signal name="5V">
<contactref element="5V_EXT" pad="6"/>
<contactref element="5V_EXT" pad="5"/>
<contactref element="5V_EXT" pad="4"/>
<contactref element="5V_EXT" pad="3"/>
<contactref element="5V_EXT" pad="2"/>
<contactref element="5V_EXT" pad="1"/>
<contactref element="78M05" pad="2"/>
<contactref element="C5O" pad="2"/>
</signal>
<signal name="DCIN">
<contactref element="D1" pad="A"/>
<contactref element="J2" pad="PWR"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
