<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="UNO_R3_SHIELD">
<description>Uno R3 Compatible Board Layout</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="1X06SMD">
</package>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Boards" package="UNO_R3_SHIELD" value="ARDUINO_R3_SHIELD"/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="4.7K"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value="4.7k"/>
<element name="U$1" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="MLX90614" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="C1" library="fab" package="C1206FAB" value="104"/>
<element name="HC05" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="R3" library="fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="N$6">
<contactref element="J1" pad="VIN"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="RES"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="IOREF"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="A3"/>
</signal>
<signal name="N$12">
<contactref element="J1" pad="A2"/>
</signal>
<signal name="N$13">
<contactref element="J1" pad="A1"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="A0"/>
</signal>
<signal name="N$19">
<contactref element="J1" pad="D4"/>
</signal>
<signal name="N$20">
<contactref element="J1" pad="D5"/>
</signal>
<signal name="N$21">
<contactref element="J1" pad="D6"/>
</signal>
<signal name="N$22">
<contactref element="J1" pad="D7"/>
</signal>
<signal name="N$23">
<contactref element="J1" pad="D8"/>
</signal>
<signal name="N$24">
<contactref element="J1" pad="D9"/>
</signal>
<signal name="N$25">
<contactref element="J1" pad="D10"/>
</signal>
<signal name="N$26">
<contactref element="J1" pad="D11"/>
</signal>
<signal name="N$27">
<contactref element="J1" pad="D12"/>
</signal>
<signal name="N$28">
<contactref element="J1" pad="D13"/>
</signal>
<signal name="N$29">
<contactref element="J1" pad="AREF"/>
</signal>
<signal name="3.3V">
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="J1" pad="3.3V"/>
<contactref element="MLX90614" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="MLX90614" pad="4"/>
<contactref element="J1" pad="A4"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="SCL">
<contactref element="MLX90614" pad="3"/>
<contactref element="J1" pad="A5"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="KEY_NC">
<contactref element="HC05" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="HC05" pad="5"/>
<contactref element="J1" pad="5V"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="GND">
<contactref element="HC05" pad="4"/>
<contactref element="J1" pad="GND@0"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="MLX90614" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="HC05" pad="3"/>
<contactref element="J1" pad="RX"/>
</signal>
<signal name="RXD">
<contactref element="HC05" pad="2"/>
<contactref element="J1" pad="TX"/>
</signal>
<signal name="STATE_NC">
<contactref element="HC05" pad="1"/>
</signal>
<signal name="DT">
<contactref element="J1" pad="D3"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="D2"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="SDA"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="SCL"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="GND@1"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="GND@2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
