<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="2N7002-1" library="fab" package="SOT-23" value=""/>
<element name="2N7002-2" library="fab" package="SOT-23" value=""/>
<element name="2N7002-3" library="fab" package="SOT-23" value=""/>
<element name="2N7002-4" library="fab" package="SOT-23" value=""/>
<element name="HIGH_SIDE" library="SparkFun-Connectors" package="1X06_LONGPADS" value=""/>
<element name="LOW_SIDE" library="SparkFun-Connectors" package="1X06_LONGPADS" value=""/>
<element name="R9" library="fab" package="R1206FAB" value="2K"/>
<element name="R10" library="fab" package="R1206FAB" value="2K"/>
<element name="R11" library="fab" package="R1206FAB" value="2k"/>
<element name="R12" library="fab" package="R1206FAB" value="2k"/>
<element name="R13" library="fab" package="R1206FAB" value="2k"/>
<element name="R14" library="fab" package="R1206FAB" value="2k"/>
<element name="R15" library="fab" package="R1206FAB" value="2k"/>
<element name="R16" library="fab" package="R1206FAB" value=""/>
</elements>
<signals>
<signal name="LO3">
<contactref element="2N7002-3" pad="2"/>
<contactref element="LOW_SIDE" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="HI3">
<contactref element="2N7002-3" pad="1"/>
<contactref element="HIGH_SIDE" pad="5"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="LO4">
<contactref element="2N7002-4" pad="2"/>
<contactref element="LOW_SIDE" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="HI4">
<contactref element="2N7002-4" pad="1"/>
<contactref element="HIGH_SIDE" pad="6"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="2N7002-1" pad="3"/>
<contactref element="2N7002-2" pad="3"/>
<contactref element="2N7002-3" pad="3"/>
<contactref element="2N7002-4" pad="3"/>
<contactref element="LOW_SIDE" pad="4"/>
<contactref element="R9" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="HIGH_SIDE" pad="3"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="LO1">
<contactref element="2N7002-1" pad="2"/>
<contactref element="LOW_SIDE" pad="6"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="HI1">
<contactref element="2N7002-1" pad="1"/>
<contactref element="HIGH_SIDE" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="LO2">
<contactref element="2N7002-2" pad="2"/>
<contactref element="LOW_SIDE" pad="5"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="HI2">
<contactref element="2N7002-2" pad="1"/>
<contactref element="HIGH_SIDE" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="GND">
<contactref element="LOW_SIDE" pad="3"/>
<contactref element="HIGH_SIDE" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
