<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.508" x2="32.436" y2="-0.635" width="0" layer="20"/>
<wire x1="32.436" y1="-0.635" x2="32.436" y2="61.331" width="0" layer="20"/>
<wire x1="32.436" y1="61.331" x2="0" y2="61.458" width="0" layer="20"/>
<wire x1="0" y1="61.458" x2="0" y2="-0.508" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LA" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="LB" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="LC" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="LD" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="LE" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="LF" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="LG" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="RA" library="fab" package="R1206FAB" value=""/>
<element name="RB" library="fab" package="R1206FAB" value=""/>
<element name="RC" library="fab" package="R1206FAB" value=""/>
<element name="RD" library="fab" package="R1206FAB" value=""/>
<element name="RE" library="fab" package="R1206FAB" value=""/>
<element name="RF" library="fab" package="R1206FAB" value=""/>
<element name="RG" library="fab" package="R1206FAB" value=""/>
<element name="U$17" library="fab" package="SOIC8" value="ATTINY45SI"/>
<element name="U$3" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="R1" library="fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$17" pad="8"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U$17" pad="4"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U$17" pad="1"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$17" pad="5"/>
<contactref element="U$3" pad="6"/>
<contactref element="LD" pad="1"/>
<contactref element="LE" pad="1"/>
<contactref element="LF" pad="1"/>
<contactref element="RC" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U$17" pad="6"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="U$17" pad="7"/>
<contactref element="LA" pad="1"/>
<contactref element="LB" pad="1"/>
<contactref element="LC" pad="1"/>
<contactref element="RF" pad="2"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="PB4">
<contactref element="RA" pad="2"/>
<contactref element="RD" pad="2"/>
<contactref element="RG" pad="2"/>
<contactref element="U$17" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="LA" pad="2"/>
<contactref element="RA" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LB" pad="2"/>
<contactref element="RB" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="LC" pad="2"/>
<contactref element="RC" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="LD" pad="2"/>
<contactref element="RD" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="LE" pad="2"/>
<contactref element="RE" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="LF" pad="2"/>
<contactref element="RF" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="LG" pad="2"/>
<contactref element="RG" pad="1"/>
</signal>
<signal name="PB3">
<contactref element="U$17" pad="2"/>
<contactref element="LG" pad="1"/>
<contactref element="RB" pad="2"/>
<contactref element="RE" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
