<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="-5.08" x2="100" y2="-5.08" width="0" layer="20"/>
<wire x1="100" y1="-5.08" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="-5.08" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="2X03SMD">
</package>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FTDI_BASIC">
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="LED_LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
</packages>
</library>
<library name="esp8266modules">
<packages>
<package name="ESP12-SMD">
<description>ESP8266 Module 12 SMD pads</description>
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="UX60-MB-5S8">
<description>&lt;b&gt;MINI USB Connector HI-SPEED Certified&lt;/b&gt; Metal Shield Dip Type With Positioning Post&lt;p&gt;
Source: http://www.hirose.co.jp/cataloge_hp/e24000019.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="C2" library="fab" package="C1206FAB" value="10uf"/>
<element name="C3" library="fab" package="C1206FAB" value="1uf"/>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="IC3" library="linear" package="SOT223" value="317EMP"/>
<element name="JP2" library="SparkFun-Connectors" package="FTDI_BASIC" value="FTDI_BASICPTH"/>
<element name="LED1" library="eagle-ltspice" package="LED_LD260" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="SPICETYPE" value="diode"/>
</element>
<element name="LED2" library="eagle-ltspice" package="LED_LD260" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="SPICETYPE" value="diode"/>
</element>
<element name="R1" library="fab" package="R1206W" value="10K"/>
<element name="R2" library="fab" package="R1206W" value="10K"/>
<element name="R3" library="fab" package="R1206W" value="10K"/>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$2" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="U1" library="esp8266modules" package="ESP12-SMD" value=""/>
<element name="X1" library="con-hirose" package="UX60-MB-5S8" value="MINI-USB-UX60-MB-5S8">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
</elements>
<signals>
<signal name="MISO">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="5"/>
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="VCC"/>
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="U1" pad="VCC"/>
<contactref element="U1" pad="RESET"/>
<contactref element="U1" pad="CH_PD"/>
<contactref element="U1" pad="GPIO0"/>
<contactref element="U1" pad="GPIO2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="JP2" pad="GND"/>
<contactref element="U$2" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="X1" pad="5"/>
<contactref element="IC3" pad="1"/>
<contactref element="U1" pad="GND"/>
<contactref element="U1" pad="GPIO15"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="RX">
<contactref element="IC1" pad="12"/>
<contactref element="JP2" pad="RXI"/>
<contactref element="U1" pad="RXD0"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="13"/>
<contactref element="JP2" pad="TXO"/>
<contactref element="U1" pad="TXD0"/>
</signal>
<signal name="XTAL1">
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="XTAL2">
<contactref element="U$2" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="MICROUSBVCC">
<contactref element="X1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="C2" pad="1"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="RED_LED">
<contactref element="LED1" pad="A"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="GREEN_LED">
<contactref element="LED2" pad="A"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$4">
<contactref element="IC3" pad="4"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
