<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="38" y1="41.5" x2="81" y2="41.5" width="0" layer="20"/>
<wire x1="81" y1="41.5" x2="81" y2="76" width="0" layer="20"/>
<wire x1="81" y1="76" x2="38" y2="76" width="0" layer="20"/>
<wire x1="38" y1="76" x2="38" y2="41.5" width="0" layer="20"/>
<hole x="42" y="71" drill="3"/>
<hole x="42" y="46" drill="3"/>
<hole x="77" y="58.5" drill="3"/>
<hole x="43.125" y="52.925" drill="1"/>
<hole x="43.125" y="50.4" drill="1"/>
<hole x="47.175" y="69.6" drill="1"/>
<hole x="49.725" y="69.6" drill="1"/>
<hole x="52.275" y="69.6" drill="1"/>
<hole x="54.8" y="69.6" drill="1"/>
<hole x="57.375" y="69.6" drill="1"/>
<hole x="72.125" y="72" drill="1"/>
<hole x="72.125" y="69.2" drill="1"/>
<hole x="72.125" y="66.4" drill="1"/>
<hole x="74.65" y="66.4" drill="1"/>
<hole x="74.65" y="69.2" drill="1"/>
<hole x="74.65" y="72" drill="1"/>
<hole x="77.2" y="72" drill="1"/>
<hole x="77.2" y="69.2" drill="1"/>
<hole x="77.2" y="66.4" drill="1"/>
<hole x="72" y="60.65" drill="1"/>
<hole x="72" y="58.125" drill="1"/>
<hole x="72.025" y="55.575" drill="1"/>
<hole x="65.925" y="47.6" drill="1"/>
<hole x="63.025" y="47.575" drill="1"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X04_NO_SILK_ALL_ROUND">
</package>
<package name="1X03">
</package>
<package name="1X02_LOCK">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="10uF"/>
<element name="C2" library="fab" package="C1206FAB" value="100nF"/>
<element name="D1" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="J1" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="R2" library="fab" package="R1206FAB" value="100"/>
<element name="U$1" library="fab" package="SOT223" value="REG-3.3-NOSTRO"/>
<element name="U$2" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="J4" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="J5" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="J6" library="SparkFun-Connectors" package="1X02_LOCK" value=""/>
<element name="J7" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="J8" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="R3" library="fab" package="R1206FAB" value="100"/>
<element name="D2" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="R4" library="fab" package="R1206FAB" value="100"/>
<element name="D3" library="SparkFun-LED" package="LED-1206" value=""/>
</elements>
<signals>
<signal name="VEXT">
<contactref element="U$1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="18"/>
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="29"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="7"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="8"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="TX">
<contactref element="J2" pad="3"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="RX">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="POT1">
<contactref element="U1" pad="23"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="POT2">
<contactref element="U1" pad="24"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="POT3">
<contactref element="U1" pad="25"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="BTN1">
<contactref element="J6" pad="2"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="MOSI">
<contactref element="J7" pad="1"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="MISO">
<contactref element="J7" pad="2"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="J7" pad="3"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="LED1">
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="LED2">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
