<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="76.18" y2="0" width="0" layer="20"/>
<wire x1="76.18" y1="0" x2="76.18" y2="31.42" width="0" layer="20"/>
<wire x1="76.18" y1="31.42" x2="0" y2="31.42" width="0" layer="20"/>
<wire x1="0" y1="31.42" x2="0" y2="0" width="0" layer="20"/>
<hole x="15.24" y="10.16" drill="1"/>
<hole x="15.24" y="12.7" drill="1"/>
<hole x="15.24" y="15.24" drill="1"/>
<hole x="9.290540625" y="11.638746875" drill="1"/>
<hole x="6.75594375" y="11.638746875" drill="1"/>
<hole x="45.72" y="3.81" drill="1"/>
<hole x="48.26" y="3.81" drill="1"/>
<hole x="50.8" y="3.81" drill="1"/>
<hole x="53.34" y="3.81" drill="1"/>
<hole x="55.88" y="3.81" drill="1"/>
<hole x="58.42" y="3.81" drill="1"/>
<hole x="60.96" y="3.81" drill="1"/>
<hole x="63.5" y="3.81" drill="1"/>
<hole x="40.64" y="7.62" drill="1"/>
<hole x="40.64" y="10.16" drill="1"/>
<hole x="40.64" y="12.7" drill="1"/>
<hole x="40.64" y="15.24" drill="1"/>
<hole x="68.58" y="7.62" drill="1"/>
<hole x="68.58" y="10.16" drill="1"/>
<hole x="68.58" y="12.7" drill="1"/>
<hole x="68.58" y="15.24" drill="1"/>
<hole x="68.58" y="17.78" drill="1"/>
<hole x="68.58" y="20.32" drill="1"/>
<hole x="68.58" y="25.4" drill="1"/>
<hole x="66.04" y="25.4" drill="1"/>
<hole x="63.5" y="25.4" drill="1"/>
<hole x="60.96" y="25.4" drill="1"/>
<hole x="58.42" y="25.4" drill="1"/>
<hole x="55.88" y="25.4" drill="1"/>
<hole x="53.34" y="25.4" drill="1"/>
<hole x="50.8" y="25.4" drill="1"/>
<hole x="48.26" y="25.4" drill="1"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="USB_MINIB">
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK_ALL_ROUND">
</package>
<package name="1X09_NO_SILK">
</package>
<package name="1X06_NO_SILK">
</package>
<package name="1X08_PIN1_NO_SILK">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1@100NF" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="C2@10UF" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="C3@100NF" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="C4@10UF" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="C5@100NF" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="D1" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X09_NO_SILK" value=""/>
<element name="J5" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X08_PIN1_NO_SILK" value=""/>
<element name="JP1" library="fab" package="2X03SMD" value=""/>
<element name="R1" library="fab" package="R1206FAB" value=""/>
<element name="R2" library="fab" package="R1206FAB" value=""/>
<element name="R3" library="fab" package="R1206FAB" value=""/>
<element name="R4" library="fab" package="R1206FAB" value=""/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="U$1" library="atmel" package="TQFP32-08" value="XMEGA8E5"/>
<element name="U$2" library="fab" package="USB_MINIB" value="USB_MINIB"/>
<element name="U$3" library="fab" package="SOT223" value="REG-3.3-NOSTRO"/>
<element name="R5" library="fab" package="R1206FAB" value=""/>
<element name="J7" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="J1" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="D2" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="R6" library="fab" package="R1206FAB" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="C1@100NF" pad="1"/>
<contactref element="U$3" pad="3"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="GND"/>
<contactref element="C1@100NF" pad="2"/>
<contactref element="C2@10UF" pad="2"/>
<contactref element="C4@10UF" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="C3@100NF" pad="2"/>
<contactref element="U$1" pad="18"/>
<contactref element="R2" pad="1"/>
<contactref element="C5@100NF" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="R4" pad="2"/>
<contactref element="J5" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="VBUS"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="J7" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="C2@10UF" pad="1"/>
<contactref element="C3@100NF" pad="1"/>
<contactref element="U$1" pad="17"/>
<contactref element="U$1" pad="32"/>
<contactref element="C4@10UF" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="J5" pad="3"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="4"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="R1" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="C5@100NF" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="JP1" pad="5"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="S1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="7"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="D1" pad="C"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="3"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="4"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="5"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="6"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="31"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="30"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="29"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="28"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="27"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="26"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="25"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="24"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="23"/>
<contactref element="J4" pad="9"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="22"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="21"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="9"/>
<contactref element="J6" pad="8"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="10"/>
<contactref element="J6" pad="7"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="11"/>
<contactref element="J6" pad="6"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="12"/>
<contactref element="J6" pad="5"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="13"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="N$28">
<contactref element="U$1" pad="14"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="15"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="U$1" pad="16"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="R5" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="R6" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
