<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<hole x="100.35" y="54.3" drill="1.2"/>
<hole x="100.35" y="50.8" drill="1.2"/>
<hole x="92.71" y="49.53" drill="1"/>
<hole x="92.71" y="52.07" drill="1"/>
<hole x="92.71" y="54.61" drill="1"/>
<hole x="90.17" y="54.61" drill="1"/>
<hole x="90.17" y="52.07" drill="1"/>
<hole x="90.17" y="49.53" drill="1"/>
<hole x="87.63" y="49.53" drill="1"/>
<hole x="87.63" y="52.07" drill="1"/>
<hole x="87.63" y="54.61" drill="1"/>
<hole x="63.5" y="58.42" drill="1"/>
<hole x="66.04" y="58.42" drill="1"/>
<hole x="68.58" y="58.42" drill="1"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="D1" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="J1" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="J4" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JP1" library="fab" package="2X03SMD" value=""/>
<element name="R1" library="fab" package="R1206FAB" value=""/>
<element name="R2" library="fab" package="R1206FAB" value=""/>
<element name="U$1" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="J5" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="R3" library="fab" package="R1206FAB" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="C1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="3"/>
<contactref element="JP1" pad="6"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="J4" pad="2"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$10">
</signal>
</signals>
</board>
</drawing>
</eagle>
