•	no more than 60% power
•	decrease size = decrease speed (no more than 60%)
•	.001 cut line (cutting)
•	raster = engraving
•	vector = outline (low power 3%-7%)
•	Adobe Illustrator 5
•	stop button = pause
•	green = go (make sure door is fully shut)
•	power top button on left
•	reset 1 = resend job
•	reset 2 = confirmation tool
•	pointer = laser
•	x,y off > go > unlocks arm > use left and right tab to move head 
•	set home center > reset > new home set
•	back to 0,0 > turn off > turn on

•	focus
•	easy = brand new material > hit focus > table moves up and down > use focus plate > set depth > hit reset
•	advanced = used material > x/y off > go > move arm > focus plate > raise bed > take off plate > reset
•	setting home
•	pointer > x/y off > dot close to edge of material > set home > reset (nothing should happen, if arm moves you did not press "set home"
•	24" x 18" is bed size
•	resolution doubles time 600 graphically = 1200 seconds vs 75 graphically = 12 seconds
•	60 watt lasers
•	300 + wont see dithering
•	shapes within shapes = inside out
•	everything else = optimize
•