<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0.0508" y1="0.0254" x2="45.4916" y2="0.0254" width="0" layer="20"/>
<wire x1="45.4916" y1="0.0254" x2="45.4916" y2="39.36" width="0" layer="20"/>
<wire x1="45.4916" y1="39.36" x2="0.0508" y2="39.3346" width="0" layer="20"/>
<wire x1="0.0508" y1="39.3346" x2="0.0508" y2="0.0254" width="0" layer="20"/>
</plain>
<libraries>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="0001_alejandro">
<packages>
<package name="RELAY-V23092">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SL1" library="con-amp-quick" package="03P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C1" library="01_SparkFun" package="CPOL-RADIAL-10UF-25V" value=""/>
<element name="U$3" library="01_FAB_Hello" package="1206" value=""/>
<element name="U$4" library="01_FAB_Hello" package="1206" value=""/>
<element name="R1" library="01_FAB_Hello" package="1206" value="1M"/>
<element name="R2" library="01_FAB_Hello" package="1206" value="1M"/>
<element name="SL4" library="con-amp-quick" package="03P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$1" library="0001_alejandro" package="RELAY-V23092" value="RELAY-V23092THROUGH_HOLE"/>
<element name="U$2" library="0001_alejandro" package="RELAY-V23092" value="RELAY-V23092THROUGH_HOLE"/>
<element name="SL2" library="con-amp-quick" package="03P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="12V">
<contactref element="SL1" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="RELAY1O">
<contactref element="SL1" pad="3"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="RELAY2O">
<contactref element="SL1" pad="1"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="12H">
<contactref element="C1" pad="1"/>
<contactref element="SL4" pad="3"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="GNDH">
<contactref element="C1" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="SL4" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="RED">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="SL2" pad="3"/>
</signal>
<signal name="BLACK">
<contactref element="R2" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="SL2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$4" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
