<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="8.19431875" y1="64.1043" x2="8.19431875" y2="0.216540625" width="0.001" layer="20"/>
<wire x1="8.19431875" y1="0.216540625" x2="0.30656875" y2="0.216540625" width="0.001" layer="20"/>
<wire x1="0.30656875" y1="0.216540625" x2="0.30656875" y2="64.1043" width="0.001" layer="20"/>
<wire x1="0.30656875" y1="64.1043" x2="8.19431875" y2="64.1043" width="0.001" layer="20"/>
<hole x="4.318" y="3.556" drill="1.4"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="allegro">
<description>&lt;b&gt;Allegro MicroSystems, Inc&lt;/b&gt;&lt;p&gt;
www.allegromicro.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-W">
<description>&lt;b&gt;3-pin SOT23W&lt;/b&gt; LH&lt;p&gt;
Source: http://www.allegromicro.com/en/Products/Packaging/pkgso2.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X2_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="fab" package="LED1206" value="LED"/>
<element name="U$2" library="fab" package="LED1206" value="LED"/>
<element name="U$3" library="fab" package="LED1206" value="LED"/>
<element name="U$4" library="fab" package="LED1206" value="LED"/>
<element name="IC1" library="allegro" package="SOT23-W" value="A1301LH">
<attribute name="MF" value="ALLEGRO MICROSYSTEMS, INC."/>
<attribute name="OC_NEWARK" value="31K6634"/>
<attribute name="OC_FARNELL" value="1198084"/>
<attribute name="MPN" value="A1301ELHLT-T"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="MOLEX-1X2_LOCK" value=""/>
<element name="J2" library="SparkFun-Connectors" package="MOLEX-1X2_LOCK" value=""/>
<element name="R1" library="fab" package="R1206FAB" value="100"/>
<element name="R2" library="fab" package="R1206FAB" value="0"/>
<element name="R3" library="fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="J2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="IC1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$4" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
