<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="34.8288" y2="0" width="0" layer="20"/>
<wire x1="34.8288" y1="0" x2="34.8288" y2="32.1312" width="0" layer="20"/>
<wire x1="34.8288" y1="32.1312" x2="0" y2="32.1312" width="0" layer="20"/>
<wire x1="0" y1="32.1312" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.4384" y="29.6672" drill="2.9972"/>
<hole x="32.512" y="29.6672" drill="2.9972"/>
<hole x="32.1056" y="2.4384" drill="2.9972"/>
<hole x="2.4384" y="2.4384" drill="2.9972"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="2X02SMD">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="EAGLE-BOARD-TO-BOARD_CONNECTORS-rev16c">
<description>&lt;BR&gt;Wurth Elektronik - Board to Board Connectors&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2016c, 2016-09-30
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="61000618221">
<description>WR-PHD 2.54mm SMT Pin Header, 6 Pins</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1u"/>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="T1" library="fab" package="SOT-23" value=""/>
<element name="T2" library="fab" package="SOT-23" value=""/>
<element name="T3" library="fab" package="SOT-23" value=""/>
<element name="T4" library="fab" package="SOT-23" value=""/>
<element name="U$2" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="J1" library="EAGLE-BOARD-TO-BOARD_CONNECTORS-rev16c" package="61000618221" value=""/>
<element name="IC2" library="fab" package="SOT23" value=""/>
</elements>
<signals>
<signal name="T3">
<contactref element="IC1" pad="11"/>
<contactref element="T3" pad="3"/>
</signal>
<signal name="T4">
<contactref element="IC1" pad="10"/>
<contactref element="T4" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="U$1" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="T1" pad="2"/>
<contactref element="T2" pad="2"/>
<contactref element="T3" pad="2"/>
<contactref element="T4" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="5"/>
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="T1">
<contactref element="IC1" pad="13"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="T2">
<contactref element="IC1" pad="12"/>
<contactref element="T2" pad="3"/>
</signal>
<signal name="TX">
<contactref element="U$2" pad="4"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="RX">
<contactref element="U$2" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="T1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="T2" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="T3" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="T4" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="VIN">
<contactref element="IC2" pad="2"/>
<contactref element="J1" pad="5"/>
<contactref element="U$2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
